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The CL range combines a step ladder and an extension ladder in one product. Offering the following features:
· Unique sliding mechanism for easy conversion to all combinations.
· Wide base and heavy duty feet for stability and grip.
· Compact folded dimensions for easy transport and storage.
· Stabilisers for extra stability [mandatory on all ladders above 3m].
· Suitable for Trade and Professional use.
· Certified to EN131 standard.

Key Benefits
· Versatile Functionality: Use as an "A" frame stepladder, step ladder with extended reach, or an extension ladder, all in one tool.
· Comfortable Climbing: Strengthened D-shaped rungs provide secure and comfortable footing.
· Enhanced Safety: High-quality stabiliser bar with a larger footprint reduces sideways slips, ensuring maximum stability.
· Durable Construction: Built with premium aluminium and tested for 50,000 cycles, ensuring long-lasting use.
· Eco-Friendly: Rungs are made from UK-sourced Recycled Low-Carbon Aluminium 4.0, reducing carbon footprint.
· High Load Capacity: Supports up to 150kg, suitable for heavy-duty trade applications.
· Stairway Use: 6 and 9 tread options can be safely used on stairs.
· Professional Certification: Certified to EN131-2, ensuring quality and compliance.


CL12 Specifications:
This product was developed in 1998 in response to the growing need for a safety ladder product which would combine a lean-to ladder with an A-Frame ladder. Great care has been taken in the development of this product and today, our combination ladder is as safe as any professional extension ladder.
· Use it as a lean-to ladder or
as an A-frame self-supporting ladder.
· 6 and 9 rung units can be used on stairwells

	Order Code
	Closed Height (m)
	Extended Stepladder Height (m)
	Extension Ladder Height (m)
	Weight
(kg)

	LCL6
	1.71
	2.43
	3.39
	9.15

	LCL9
	2.56
	4.00
	5.92
	15.10

	LCL12
	3.40
	5.59
	8.44
	23.00






[image: 3-section combination ladders - h2960mm closed height mm 2960, extended height mm 6860]
[image: transformable aluminium 3 section combination ladder no. of rungs per section 13]

	[image: 3-section combination ladders - h1800mm closed height mm 1800, extended height mm 3780]
image1.png
IE) DUBLIN
LADDERS




image2.jpeg




image3.jpeg




image4.jpeg




