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Certificate of specification & safety articles for bespoke mobile steps
All our mobile steps/Dock Steps are built to EN131-7 Standard.
General:  Although there are no recognised accreditations or certificates assigned to mild-steel Mobile steps, we maintain a high standard in the production of our safety products, which is closely aligned with established and acclaimed protocols relating to accredited steps & ladders.   The safety features of our in-house designed steps have been established and field-tested over the course of 30 years of production.  As bespoke steps are manufactured to the individual needs of the end user, more care and attention to detail is delivered than would be expected from standard production units.  Our manufacturing process is carefully monitored to ensure quality and safety; this includes careful attention to the use of top quality raw materials, welding processes, assembly and pre-delivery inspection.

Safety, stability & reliability are achieved by strict adherence to the following criteria:
1. Frame-work:  All units are built from top quality semi-bright steel [i.e. mix of iron & zinc].
2. All treads & tread plates are made of cold-rolled steel/aluminium which is resistant to fracture.
3. The rake angle of the stairwell is set at 54 degrees to shield against ‘fallback’ during ascent and descent.
4. Stability is provided by the use of cross-bracing on the back riser frame.  The step unit is further secured by a manually operated handbrake located to the front of the unit.
5. All our steps are fully welded [every joint] to ensure integrity of the frame.
6. The handrails rise 450mm [minimum] above the stairwell thus providing hazard-free usage.  
7. The wheels and castors have a minimum load-rating of 150kg per unit.
The standards set out above closely reflect [and often exceed] the criteria and norms required by many accreditation bodies of manufacturers who produce accredited products.  Under European Law, fully welded steel mobile steps are designated as ‘Machines’. 


User Safety:
1. Always apply handbrake before climbing
2. Footwear:  laced boots or factory shoes
3. Observe load rating:  150KG rated for 1 person [ Dock steps can also accommodate an additional 100KG of equipment on the platform deck].
4. Never carry equipment as you climb the Dock step; always ask another staff member to hand you tools etc as soon as you are safely on the platform.
5. The walk-off [LHS/RHS] is chain-guarded. A chain will not always prevent a fall.  It is designed to alert the user of a planned platform opening.
6. Carry out pre-use checks; visual checks include: clean surfaces, undamaged frame, operational handbrake.
7. Never reach outside of the Dock step parameters
8. Only use on level ground
9. The unit is fitted with a Ladder Tag.  Fill this in every 2 weeks.  Additional Tags can be ordered by contacting us.  



